{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":50,"n_cols":9,"rows_kept":50,"merged":[[6,0,6,1]]}
["序号","设备名称","设备参数 ","品牌","数量","单位","单价","总价","备注"]
["综合 布线"]
["工作区子系统"]
[1,"超5类非屏蔽模块",null,"大华",236,"个"]
[2,"超5类水晶头",null,"大华",5,"盒"]
[3,"数据双口面板",null,"大华",118,"个"]
["水平子系统"]
[1,"超五类非屏蔽网线",null,"大华",19000,"米"]
["垂直子系统"]
[1,"25对大对数电缆",null,"国产",640,"米"]
[2,"4芯多模万兆室内光缆",null,"国产",640,"米"]
["管理间子系统"]
[1,"机柜","550*400*600","国产",8,"套"]
[2,"超5类非屏蔽配线架",null,"国产",16,"个"]
[3,"110配线架-50对",null,"国产",8,"个"]
[4,"110配线架-100对",null,"国产",2,"个"]
[5,"1U水平理线器",null,"国产",25,"个"]
[6,"48口光纤配线架",null,"国产",1,"个"]
[7,"24口光纤配线架",null,"国产",8,"个"]
[8,"LC-LC耦合器",null,"国产",80,"个"]
[9,"1M万兆多模尾纤",null,"国产",80,"条"]
[10,"LC-LC光纤跳线",null,"国产",40,"条"]
[null,"合计"]
["有线网络系统"]
[3,"核心交换机","RG-NBS5710-24GT4SFP-E  24口10/100/1000M自适应电口，4个1G SFP光口，固化单交流电源,交换容量  336Gbps,包转发率51Mpps,MAC表项12K,支持QinQ、灵活QinQ,支持静态路由、RIP、OSPF，工作温度：0-50℃，云管平台：支持MACC免费管理；支持VSU","睿易",1,"台",null,null,"机房核心设备"]
[4,"百兆交换机","1、实配固化10/100/1000M以太网端口≥24个\n2、要求所投交换机满足交换容量≥48Gbps，转发性能≥36Mpps \n3、产品支持端口防雷≥4KV（非防静电），\n4、要求所投产品工作温度范围0-50°C，提供官网截图及链接作为证明材料\n5、产品可快速检测链路的通断，并支持端口下的环路检测功能，防止端口下因私接Hub等设备形成的环路而导致网络故障，\n6、交换机支持手机APP集中管理，能够实现拓扑呈现、端口状态显示、VLAN配置等， \n7、要求设备支持802.1Q，支持流控，端口限速，风暴抑制，端口隔离，端口镜像，并可通过WEB界面实现向导性配置","睿易",8,"台",null,null,"每层每个弱电井一台"]
["监控设备网络系统"]
[1,"核心交换","RG-NBS5710-24GT4SFP-E  24口10/100/1000M自适应电口，4个1G SFP光口，固化单交流电源,交换容量  336Gbps,包转发率51Mpps,MAC表项12K,支持QinQ、灵活QinQ,支持静态路由、RIP、OSPF，工作温度：0-50℃，云管平台：支持MACC免费管理；支持VSU\n","睿易",1,"台",null,null,"机房核心设备"]
[2,"8口百兆交换机","中文大华百兆SOHO交换机\n8个百兆电口","大华",10,"台",null,null,"一层和三层弱电井各放一台"]
["小计"]
["电视监控"]
[1,"网络高清红外半球摄像机",null,"海康",12,"个"]
[2,"网络高清红外全球摄像机（带云台）",null,"海康",48,"个"]
[3,"DH-PFB121W-普通壁装枪机支架-DH816W2-中文大华","铝合金；白色；最大承重1.0kg；壁装；","海康",60,"个"]
[4,"桌面式电源适配器-AC180V~264V-12V2A-V级-DH-PFM301-国标-安防电源v1.0-Φ5.5×Φ2.1×10","DC12V2A电源适配器","海康",60,"个"]
[5,"电源线","1.5*2","大华",4800,"个"]
[null,"合计"]
["校园广播"]
["扬声器"]
[1,"壁挂扬声器（10W/5W）","◆6\"×1低音喇叭单元.2\"×1高音单元                                           ◆音质清晰,明亮.                                                 ◆额定功率：15W.                                                    ◆输入电压：70-100V.                                               ◆灵敏度：93dB.                                            ◆频率响应:90-20KHz.                                                                            ◆尺寸：200×105×275mm。","聆霸LBG-502B",24,"台"]
["辅材部分"]
[1,"专业广播机柜","一到二个风扇；一到三个固定拖板；一个电源条。螺丝若干。静电喷塑,冷轧板制做。豪华型机柜前门玻璃,为钢化玻璃.",null,1,"套",null,null,"自购"]
["残卫呼系统"]
[1,"声光报警器","天良","TL-C-LA06",4]
[2,"呼叫按钮","天良","TL-C-EC09",4]
[3,"钥匙复位开关","天良","TL-C-CA06",4]
[4,"控制器","天良","TL-C-DT300",4]
["总计"]
[]
["合计",{"$nulls":6},{"$f":"H48+H42+H40+H37+H23","v":0}]