{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"merged":[[0,0,0,7],[1,0,1,1],[1,2,1,7],[2,3,2,4],[3,3,3,4],[4,3,4,4],[5,3,5,4],[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,3,9,4],[10,3,10,4],[11,3,11,4],[12,3,12,4],[13,3,13,4],[14,3,14,4],[15,3,15,4],[16,3,16,4],[17,3,17,4],[18,3,18,4],[19,3,19,4],[20,3,20,4],[21,3,21,4],[22,3,22,4],[23,3,23,4],[24,3,24,4],[25,3,25,4],[26,3,26,4],[27,3,27,4],[28,3,28,4],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[37,3,37,4],[38,3,38,4],[39,3,39,4],[40,3,40,4],[41,3,41,4],[42,3,42,4],[43,3,43,4],[44,3,44,4],[45,3,45,4],[46,3,46,4],[47,3,47,4],[48,3,48,4],[49,2,49,7]]}
["设备清单或工程量清单确认表"]
["采购项目名称",null,"菏泽市档案馆（含城建档案馆）智能化工程-机房装修"]
["序号","设备名称","厂家","参数",null,"单位","数量","备注"]
[null,"土建"]
[1,"机房彩钢板",null,"轻质墙板\n1.墙板材质:机房彩钢板\n2.墙板厚度:1.2mm厚",null,"m2",222.03]
[{"$f":"ROW()-4","v":2},"保温隔热天棚",null,"保温隔热天棚\n1.保温隔热面层材料品种、规格、性能：铝箔\n2.保温隔热材料品种、规格及厚度：20mm厚B1级橡塑",null,"m2",132.4]
[{"$f":"ROW()-4","v":3},"保温隔热楼地面",null,"保温隔热楼地面\n1.保温隔热部位：地面\n2.保温隔热材料品种、规格、厚度：20mm厚B1级橡塑板",null,"m2",132.4]
[4,"保温隔热墙面",null,"保温隔热墙面\r\n1.保温隔热部位：墙面\r\n2.保温隔热方式：20mm厚B1级橡塑板\r",null,"m2",148.02]
[5,"保温隔热墙面",null,"保温隔热墙面\r\n1.保温隔热部位：彩钢板龙骨内\r\n2.保温隔热方式：50mm厚岩棉板\r",null,"m2",222.03]
[null,"装饰"]
[6,"吊顶天棚",null,"吊顶天棚\n1.吊顶形式、吊杆规格、高度：平面\n2.龙骨材料种类、规格、中距：浮搁式铝合金龙骨不上人型含龙骨\n4.面层材料品种、规格：铝塑板",null,"m2",132.4]
[7,"金属装饰线",null,"金属装饰线\r\n1.基层类型：铝合金\r\n2.线条材料品种、规格、颜色：角线 30mm以内\r",null,"m",74.01]
[8,"玻璃隔断",null,"玻璃隔断\n1.边框材料种类、规格：镀锌方管\n2.玻璃品种、规格、颜色：12mm 防火玻璃\n3.嵌缝、塞口材料品种：嵌缝胶",null,"m2",27.65]
[null,"机房电气"]
[9,"照明灯",null,"普通灯具\r\n1.名称：机房普通照明灯\r\n2.型号：600*600-18W-LED\r\n3.规格：正方形罩\r\n4.类型：6500K",null,"套",19]
[10,"接线盒",null,"接线盒\n1.名称:接线盒\n2.材质:\n3.规格:\n4.安装形式:",null,"个",21]
[11,"出口指示灯",null,"装饰灯\n1.灯具名称：出口指示灯\n2.规格\n：应急时间≥90min.\n3.安装形式及高度:2.85M嵌入式安装",null,"套",6]
[12,"疏散指示灯",null,"装饰灯\r\n1.名称:疏散指示灯\r\n2.规格:应急时间≥90min.\r\n3.安装形式及高度:0.3M壁挂式安装",null,"套",5]
[13,"机房照明板式开关",null,"照明开关\n1.名称：机房照明板式开关\n2.材质：氨基模塑料\n3.规格：双联\n4.安装方式：86盒上安装",null,"个",2]
[14,"地面五孔插座",null,"插座\n1.名称：地面五孔插座\n2.材质：铜质\n3.规格：单相30A\n4.安装方式：静电地板上嵌入式安装",null,"个",3]
[15,"应急照明",null,"普通灯具\r\n1.名称：机房应急照明\r\n2.型号：600*600-18W-LED\r\n3.规格：正方形罩\r\n4.类型：6500K",null,"套",19]
[16,"抗震底座",null,"抗震底座\n1.名称：UPS主机/总输入柜/市电柜抗震底座\n2.材质：角钢\n3.规格：40*40*3MM\n4.安装方式：地面螺栓固定安装",null,"个",3]
[17,"抗震底座",null,"抗震底座\n1.名称：电池抗震底座\n2.材质：角钢\n3.规格：40*40*3MM\n4.安装方式：地面螺栓固定安装",null,"个",2]
[18,"支架",null,"设备支架制作安装\n1.名称：UPS电池组机架\n2.材质：镀锌方管\n3.支架每组质量：0.2t以内",null,"套",2]
[19,"照明板式开关",null,"照明开关\n1.名称：机房照明板式开关\n2.材质：氨基模塑料\n3.规格：单联\n4.安装方式：86盒上安装",null,"个",6]
[20,"等电位端子箱",null,"等电位端子箱、测试板\r\n1.名称:等电位端子箱\r\n2.材质:\r\n3.规格:",null,"台\r\n",2]
[21,"接地",null,"计算机应用、网络系统接地\r\n1.名称：接地跨接线\r\n2.类别：BV\r\n3.规格：4m2\r\n4.具体详见图纸设计",null,"系统",1]
[22,"接地",null,"计算机应用、网络系统接地\r\n1.名称：静电地板地网\r\n2.类别：C1100\r\n3.具体详见图纸设计\r",null,"系统",1]
[23,"五孔插座",null,"插座\n1.名称：五孔插座\n2.材质：\n3.规格：单相30A\n4.安装方式：86盒上安装",null,"个",15]
[24,"镀锌钢管",null,"配管\r\n1.名称：JDG\r\n2.材质：镀锌钢管\r\n3.规格：DN20\r\n4.配置形式：电线管砖、混凝土结构明配\r",null,"m",263]
[25,"桥架",null,"桥架\n1.名称：机房配电桥架\n2.型号：槽式\n3.规格：300*100\n4.材质：镀锌钢板静电喷塑",null,"m",28]
[26,"接地铜板",null,"计算机应用、网络系统接地\r\n1.名称：悬浮接地铜板\r\n2.类别：等电位\r\n3.规格：25*3mm\r\n4.具体详见图纸设计",null,"系统",1]
[null,"机房弱电"]
[27,"桥架",null,"桥架\r\n1.名称:桥架\r\n2.型号:300*100\r\n3.规格:\r\n4.材质:金属\r\n5.类型:\r\n6.接地方式:",null,"m",15]
[28,"镀锌钢管",null,"配管\r\n1.名称：JDG\r\n2.材质：镀锌钢管\r\n3.规格：DN20\r\n4.明敷\r\n",null,"m",55]
[29,"机柜抗震底座",null,"抗震底座\n1.名称：机柜抗震底座\n2.材质：角钢\n3.规格：40*40*3MM\n4.安装方式：地面螺栓固定安装",null,"个",6]
[null,"机房送排风"]
[30,"碳钢阀门",null,"碳钢阀门\n1.名称：70℃防火阀\n2.型号：400*300\n3.带电动执行机构\n4.其他参数详见图纸",null,"个",2]
[31,"新风风阀",null,"碳钢阀门\n1.名称：新风风阀\n2.型号：500*350\n3.带电动执行机构\n4.其他详见图纸设计",null,"个",1]
[32,"送风口",null,"碳钢风口、散流器、百叶窗\r\n1.名称:送风口\r\n2.型号:350*350\r\n3.规格:其他参数详见图纸，满足规范要求\r\n4.质量:\r\n5.类型:\r\n6.形式:",null,"个",6]
[33,"风道",null,"碳钢通风管道\n1.名称:风道\n2.材质:镀锌钢板\n3.形状:矩形\n4.规格:\n5.板材厚度:满足规范要求\n6.管件、法兰等附件及支架设计要求:\n7.接口形式:",null,"m2",42]
[34,"防火阀",null,"碳钢阀门\r\n1.名称：280℃防火阀\r\n2.型号：400*300\r\n3.带电动执行机构\r\n4.其他参数详见图纸\r",null,"个",1]
[35,"余压阀",null,"碳钢阀门\n1.名称：余压阀\n2.型号：400*300\n3.其他参数详见图纸设计",null,"个",2]
[36,"柜式消防排烟风机",null,"离心式引风机\n1.名称：柜式消防排烟风机\n2.型号：HTFC-0.55kw\n3.规格：0.55KW 排风量1800-3500m3/h\n4.含控制箱\n5.其他参数详见图纸",null,"台",1]
[37,"吊顶式新风机 ",null,"离心式通风机\n1.名称：吊顶式新风机  \n2.型号：XD25D\n3.规格：长1035mm*宽760mm*高460mm风量 2500m3/h \n4.含控制箱\n5.其他参数详见图纸",null,"台",1]
[null,"增加"]
[38,"防静电地板",null,"防静电地板（189+113+76）",null,"m2",378]
[null,"踢脚线",{"$nulls":3},"米",150]
[null,"单扇玻璃门",{"$nulls":3},"个",2]
[null,"说明","因机房实际面积与清单不符，并甲方要求部分变更，结算时以实际面积为准。"]